For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front wheelhouse liners. Refer to Front Wheelhouse Liner Replacement.
3. Remove the front air deflector to front bumper fascia retaining screws (2).
4. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
5. Remove the front air deflector to front frame push-in retainers (3).
6. Remove the front air deflector (1).

### Installation Procedure

1. Position the front air deflector (1) to the vehicle.
2. Install the front air deflector to front frame push-in retainers (3).
3. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement.
4. Install the front air deflector to front bumper fascia retaining screws (2)

Tighten
Tighten the screws to 3 N·m (27 lb in).

5. Install the front wheelhouse liners. Refer to Front Wheelhouse Liner Replacement.
6. Lower the vehicle.