For 1990-2009 cars

### Removal Procedure

1. Remove the cylinder head. Refer to Cylinder Head Replacement - Left Side or Cylinder Head Replacement - Right Side.
2. Remove the valve lifters. Refer to Valve Lifter Removal.

### Installation Procedure

1. Install the valve lifters. Refer to Valve Lifter Installation.
2. Install the cylinder head. Refer to Cylinder Head Replacement - Left Side or Cylinder Head Replacement - Right Side.