For 1990-2009 cars

## Fastener Tightening Specifications RHD

### Fastener Tightening Specifications (3.6L Engine)

Application | Specification
--- | ---
Metric | English
Bleeder Assembly Bleed Nipple | 8 N·m | 71 lb in
Clutch Master Cylinder to Clutch Pedal Retaining Bolts | 25 N·m | 18 lb ft
Clutch Fluid Reservoir Bracket to Brake Master Cylinder End Brace Retaining Bolt | 10 N·m | 89 lb in
Clutch Fluid Reservoir to Clutch Master Cylinder Bracket Retaining Nut |  |
Clutch Pedal to Instrument Panel Crossmember Upper Retaining Bolts | 25 N·m | 18 lb ft
Clutch Pedal to Mod Plate Retaining Nuts | 22 N·m | 16 lb ft
Concentric Actuator Cylinder to Transmission Retaining Bolts | 17 N·m | 13 lb ft
Concentric Actuator Cylinder Feed Pipe Bracket to Transmission Retaining Bolt | 3 N·m | 27 lb in
Concentric Actuator Cylinder Feed Pipe to Transmission Retaining Bolt | 3 N·m | 27 lb in
Clutch Pedal Position Switch Retaining Bolt | 13 N·m | 115 lb in
Hydraulic Clutch Hose/Pipe Retaining Bolt |  |
Pressure Plate to Flywheel Retaining Bolts - First Pass Pressure Plate to Flywheel Retaining Bolts - Second Pass | 15 N·m 30 N·m | 11 lb ft 22 lb ft

### Fastener Tightening Specifications (6.0L Engine)

Application | Specification
--- | ---
Metric | English
Clutch Master Cylinder to Clutch Pedal Retaining Bolts | 12 N·m | 106 lb in
Clutch Fluid Reservoir Bracket to Brake Master Cylinder End Brace Bolt | 10 N·m | 89 lb in
Clutch Fluid Reservoir to Clutch Master Cylinder Bracket Nut | 3 N·m | 27 lb in
Clutch Pedal to Instrument Panel Crossmember Upper Retaining Bolts | 25 N·m | 18 lb ft
Clutch Pedal to Mod Plate Retaining Nuts | 22 N·m | 16 lb ft
Concentric Actuator Cylinder Bleed Screw | 18 N·m | 13 lb ft
Concentric Actuator Cylinder to Transmission Retaining Bolts | 10 N·m | 89 lb in
Concentric Actuator Cylinder Feed Pipe | 13 N·m | 10 lb in
Clutch Pedal Position Sensor Retaining Bolt | 13 N·m | 115 lb in
Pressure Plate to Flywheel Retaining Bolts - First Pass Pressure Plate to Flywheel Retaining Bolts - Second Pass Pressure Plate to Flywheel Retaining Bolts - Third Pass Pressure Plate to Flywheel Retaining Bolts - Fourth Pass | 15 N·m 35 N·m 55 N·m 70 N·m | 11 lb ft 26 lb ft 41 lb ft 52 lb ft