For 1990-2009 cars

## Floor Rear Air Outlet Duct Replacement - Left Side RHD

### Removal Procedure

1. Remove the centre console. Refer to Front Floor Console Replacement.
2. Remove the front carpet. Refer to Front Floor Panel Carpet Replacement.
3. Remove the push pin (1) from the rear floor air outlet duct (2).
4. Remove the rear floor air outlet duct (1) from the floor (2).
5. Disconnect the rear floor air outlet duct (2) from the HVAC module assembly (1).

### Installation Procedure

1. Install the rear floor air outlet duct (2) to the HVAC module assembly (1).
2. Install the rear floor air outlet duct (1) to the floor (2).
3. Install the push pins (1) to the rear floor air outlet duct (2).
4. Install the centre console. Refer to Front Floor Console Replacement.
5. Install the front carpet. Refer to Front Floor Panel Carpet Replacement.