For 1990-2009 cars

### Removal Procedure

1. Remove the positive crankcase ventilation (PCV) hose (2) from the air cleaner duct resonator (4).
2. Remove the air cleaner duct to throttle body retaining clamp (1).
3. Remove the air cleaner duct to air cleaner assembly clamp (3)
4. Remove the air cleaner duct (4).

### Installation Procedure

1. Install the air cleaner intake duct (4) to the engine.

Notice: Refer to Fastener Notice in the Preface section.

2. Tighten the air cleaner duct clamps.
3. Install the air cleaner duct to throttle body retaining clamp (1).

Tighten
Tighten the air cleaner duct clamps to 4 N·m (35 lb in).

4. Install the air cleaner duct to air cleaner assembly clamp (3)

Tighten
Tighten the air cleaner duct clamps to 4 N·m (35 lb in).

5. Install the PCV hose (2) to the intake duct resonator.