For 1990-2009 cars

### Removal Procedure

1. Remove the endgate liner. Refer to Pickup Box Endgate Liner Replacement.
2. Remove the endgate latch assembly to endgate retaining screws (3).

Important: Extend the endgate latch assembly (2) away from the endgate and slide the endgate overslam bumper (1) off the endgate latch assembly (2).

3. Remove the endgate overslam bumper (1) from the endgate latch assembly (2).

### Installation Procedure

Important: Extend the endgate latch assembly (2) away from the endgate and slide the endgate overslam bumper (1) onto the endgate latch assembly (2).

1. Install the endgate overslam bumper (1) to the endgate latch assembly (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the endgate latch assembly to endgate retaining screws (3).

Tighten
Tighten the screws to 25 N·m (18 lb ft).

3. Install the endgate liner. Refer to Pickup Box Endgate Liner Replacement.