For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Caliper Anchor Plate to Knuckle Retaining Bolts | 110 N·m | 81 lb ft
Front Subframe to Body Centre Retaining Bolts | 160 N·m | 118 lb ft
Front Subframe to Body Front Retaining Bolts | 160 N·m | 118 lb ft
Front Subframe to Body Rear Retaining Bolts | 240 N·m | 178 lb ft
I-Link to Knuckle Retaining Bolt | 140 N·m | 103 lb ft
I-Link to Rear Subframe Retaining Bolt and Nut | 175N·m | 129 lb ft
Lower Control Arm to Knuckle Retaining Bolt and Nut

- First Pass

40 N·m

30 lb ft

- Final Pass

120 Degrees

Lower Control Arm to Rear Subframe Retaining Bolt | 175 N·m | 129 lb ft
Lower Engine Mount to Front Subframe Retaining Nut | 80 N·m | 59 lb ft
Rear Subframe Retaining Bolts to Body
First Pass: | 65 N·m | 48 lb ft
Second Pass: | 125 Degrees
Steering Gear to Front Sub Frame Retaining Bolts | 65 N·m | 48 lb ft
Strut Assembly to Body Retaining Bolts | 58 N·m | 43 lb ft
Transmission Support Retaining Bolts | 58 N·m | 43 lb ft
Transmission Support to Transmission Mount Retaining Nuts (Except 5L40 and 6L50) | 25 N·m | 18 lb ft
Transmission Support to Transmission Mount Retaining Nuts (5L40 and 6L50) | 58 N·m | 43 lb ft
Upper Control Arm Ball Joint to Subframe Retaining Bolt and Nut

- First Pass

80 N·m

59 lb ft

- Final Pass

120 Degrees

Upper Control Arm Pivot Bushing to Upper Control Arm Retaining Bolt | 170 N·m | 126 lb ft
Upper Control Arm to Knuckle Retaining Bolt and Nut
First Pass: | 60 N·m | 44 lb ft
Second Pass: | 90 Degrees
Y-Link to Knuckle Retaining Bolt and Nut

- First Pass

40 N·m

30 lb ft

- Final Pass

120 Degrees

Y-Link to Rear Subframe Retaining Bolt and Nut | 175 N·m | 129 lb ft