For 1990-2009 cars

### Removal Procedure

1. Remove the centre pillar lower trim. Refer to Center Pillar Lower Trim Panel Replacement .
2. Remove the seat belt lower anchor bolt cover (2) and remove the lower anchor bolt assembly (1).
3. Remove the centre pillar upper trim panel to body retaining screws (1).
4. Using a suitable tool, prise the centre pillar upper trim panel retaining screw cover (1) from the centre pillar upper trim panel (3).
5. Remove the centre pillar upper trim panel to body retaining screw (2).
6. Remove the centre pillar upper trim panel (3) from the centre pillar.

### Installation Procedure

1. Install the centre pillar upper trim panel (3) to the centre pillar.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the centre pillar upper trim panel to body retaining screw (2).

Tighten
Tighten the retaining screw to 2.0 N·m (18 lb in).

3. Install the centre pillar upper trim panel retaining screw cover (1) to the centre pillar upper trim panel (3).
4. Install the centre pillar upper trim panel to body retaining screws (1).

Tighten
Tighten the retaining screws to 2.0 N·m (18 lb in).

5. Install the seat belt lower anchor bolt assembly (1).

Tighten
Tighten the front seat belt lower anchor bolt assembly to 43 N·m (32 lb ft).

6. Install the centre pillar lower trim. Refer to Center Pillar Lower Trim Panel Replacement .