For 1990-2009 cars

1. Remove oil jet to cylinder block retaining bolts (2).
2. Remove the oil jets (1).
3. Remove the right front oil pan rail oil gallery expansion plug (1).
4. Remove the cylinder block-to-oil pan alignment dowels (1).
5. Remove the M14 right side oil gallery threaded plug (1).
6. Remove the M14 right side coolant drain threaded plug (1).
7. Remove the M14 rear oil gallery threaded plug (1).
8. Remove the M14 left side coolant drain threaded plug (1).
9. Remove the M20 left side oil gallery threaded plug (1).
10. Remove the coolant expansion plugs (1).
11. Remove the cylinder block-to-transmission alignment dowels (1).
12. Remove the front oil gallery expansion plug (1).
13. Remove the cylinder block-to-cylinder head alignment dowels (2).