For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Install the 1-2-3-4 and 3-5 reverse clutch housing with the 1-2-3-4 clutch plates installed, onto the torque converter housing.
2. Install the DT 47868-2 onto the torque converter housing.
3. Install DT 47868-1 D onto the 1-2-3-4 clutch backing plate.
4. Install the J 26900-13 J onto DT 47868-2 .
5. Attach the J 8001 to the J 26900-13 and zero out the dial indicator on the DT 47868-1 .

#### Special Tools

• | DT 47868-1 Clutch Pack Travel Weight

• | DT 47868-2 Magnetic Base Adapter

• | J 8001 Dial Indicator Set

• | J 26900-13 Magnetic Base

1 | 1-2-3-4 Clutch Apply Passage Tip Apply compressed air to the apply passage hole, at least 3 times and observe the dial indicator measurement each time. This action "fluffs" the clutch plates to make sure an accurate measurement. Refer to Clutch Backing Plate Retaining Ring Specifications .