For 1990-2009 cars

Description | Specifications
--- | ---
Steel Wheels
Rim Width Code | 7J
Diameter Code | 16
Maximum Permissible Radial runout All Steel Wheels | 0.7 mm
Offset | 43 mm (positive)

### Alloy Wheel Specifications

Description | Specifications
--- | ---
Alloy Wheels
Rim Width Code | 8J
Diameter Code | 18, 19
Maximum Permissible Radial runout All Models | 0.4 mm
Offset
18" x 8", 19" x 8" | 48 mm (positive)

### Inflation Pressure Specifications

Model | Engine | Wheel | Tire Designation | Recommended Cold Inflation kPa
--- | --- | --- | --- | ---
Up to 3 Passengers | Up to Max. Load
Front | Rear | Front | Rear
Ute | V6 | 7J x 16 steel | 225/60 R16 102H | 250 | 250 | 270 | 300.
SV6 | V6 | 8J x 18 alloy | 245/45 R18 96V | 250 | 250 | 250 | 270
SS | V8 | 8J x 18 alloy | 245/45 R18 96V | 250 | 250 | 250 | 270
SS-V | V8 | 8J x 19 alloy | 245/40 R19 94W | 250 | 250 | 250 | 270
Temporary use spare | 17 x 4 | T155/80 R17 111M | 420