For 1990-2009 cars

### Removal Procedure

Important: Detach the engine cover to fuel rail retaining clips (1) by pulling upward on the engine cover.

1. Detach the engine cover from the fuel rail retaining clips (1).
2. Remove the engine cover (2).

### Installation Procedure

1. Align the engine cover to fuel rail retaining clips (1).

Important: Make sure the engine cover retaining clips (1) are fully engaged to prevent causing an induced rattle condition.

2. Install the engine cover (2).