For 1990-2009 cars

### Removal Procedure

1. Remove the fuel filler door. Refer to Fuel Tank Filler Door Replacement .
2. Using a suitable tool, detach the fuel cap cable retaining lug (3).
3. Remove the fuel filler door hinge to body retaining screws (1).
4. Remove the fuel filler door hinge (2) from the body (4).

### Installation Procedure

1. Position the fuel filler door hinge (2) to the body (4)

Notice: Refer to Fastener Notice in the Preface section.

2. Install the fuel filler door hinge to body retaining screws (1).

Tighten
Tighten the bolts to 2 N·m (18 lb in).

3. Attach the fuel cap cable retaining lug (3).
4. Install the fuel filler door. Refer to Fuel Tank Filler Door Replacement .