For 1990-2009 cars

Important: Follow the procedure sequence in order to prevent drive belt mis-alignment and/or possible damage/distortion to the components.

1. Install the A/C compressor bracket (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the A/C compressor bracket to cylinder block retaining bolts (1).

Tighten
Tighten the bolt to 58 N·m (42 lb ft).

3. If you are replacing the compressor, balance the compressor oil. Refer to Air Conditioning Compressor Oil Balancing.
4. Install the A/C compressor (2).
5. Install the A/C compressor to A/C compressor bracket retaining bolts (1).

Tighten
Tighten the nuts to 22 N·m (16 lb ft).