For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### Circuit/System Description

This Engine Cranks but Does Not Run diagnostic is an organized approach to identify a condition which causes the engine to crank but does not continue to run. This diagnostic directs the service technician to the appropriate system diagnosis. This diagnostic assumes the vehicle system voltage levels are adequate for starter motor operation. Refer to Battery Inspection/Test and Engine Cranks Slowly. The fuel level supply must be adequate, and the fuel quality must be able to sustain the combustion process.

### Diagnostic Aids

• | When disconnecting electrical connectors or removing fuses and relays from a fuse block, always inspect both mating electrical terminals for corrosion and terminal tightness.

• | Use the J 35616 Connector Test Adapter Kit for any test that requires probing the underhood fuse block terminals, component wire harness terminals, or the ECM wire harness terminals.

### Reference Information

#### Schematic Reference

Engine Controls Schematics

#### Connector End View Reference

Component Connector End Views

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

#### DTC Type Reference

Powertrain Diagnostic Trouble Code (DTC) Type Definitions

#### Scan Tool Reference

Control Module References for scan tool information

#### Special Tools

• | J 34730-1A Fuel Pressure Gage

• | J 35616-A/BT-8637 Connector Test Adapter Kit

• | J 43244 Relay Puller Pliers

### Circuit/System Verification

Attempt to start the engine. The engine should start and run.

⇒ | If the vehicle passes the Circuit/System Verification test, refer to Testing for Intermittent Conditions and Poor Connections.

### Circuit/System Testing

1. Crank the engine for 15 seconds.
2. Observe the vehicle DTC information with a scan tool.

⇒ | If any DTCs are set, repair those DTCs first. Refer to Diagnostic Trouble Code (DTC) List - Vehicle.

3. With the ignition ON and the engine OFF, test the fuses that are supplied ignition 1 voltage by the powertrain relay. The test lamp should illuminate ON for each test point of the fuses.

⇒ | If the test lamp does not illuminate ON for at least one test point of each fuse, refer to DTC P0685, P0689, or P0690.

4. Crank the engine for 15 seconds. Observe the engine speed parameter with a scan tool.

⇒ | If engine RPM is not indicated, refer to DTC P0335.

5. Install a spark plug tester onto one ignition module/coil assembly on each bank of the engine.
6. Observe both spark plug testers.

Important: An erratic or weak spark is considered a no spark condition.

7. Crank the engine for 15 seconds. The ignition coil secondary voltage should be observed across the gap of both spark plug testers.

⇒ | If the ignition coil secondary voltage is not observed, is inconsistent, or weak on either spark plug tester, refer to Electronic Ignition (EI) System Diagnosis.

8. With the ignition ON and the engine OFF, command the fuel pump ON and OFF with the scan tool. The fuel pump should energize when commanded ON, and de-energize when commanded OFF.

⇒ | If the fuel pump does not turn ON and OFF, refer to Fuel Pump Electrical Circuit Diagnosis.

9. Turn OFF the ignition.
10. Install the J 34730-1A Fuel Pressure Gage. With the ignition ON and the engine OFF, command the fuel pump ON several times with the scan tool. Refer to Fuel System Diagnosis for the fuel pressure specification.
11. Inspect for the following conditions:

• | Compare the actual engine coolant temperature to the ECT parameter.

• | Filter and air intake system for restrictions and obstructions

• | Test the fuel for contamination--Refer to Alcohol/Contaminants-in-Fuel Diagnosis.

• | Inspect the spark plugs--Refer to Spark Plug Inspection.

• | Test the exhaust system for restrictions--Refer to Restricted Exhaust.

• | Engine mechanical conditions, such as worn timing chain, sprocket gears, low compression, etc.--Refer to Symptoms - Engine Mechanical.

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.