For 1990-2009 cars

Notice: Refer to Fastener Notice in the Preface section.

1. Install the oil filter fitting (2).

Tighten
Tighten the fitting to 55 N·m (40 lb ft).

2. Lubricate the oil filter seal with clean engine oil.
3. Install the oil filter (2).

Tighten
Tighten the filter to 30 N·m (22 lb ft).

4. Install the oil pan drain plug (1).

Tighten
Tighten the plug to 25 N·m (18 lb ft).

5. Install the gasket (3), cover (2), and bolts (1).

Tighten
Tighten the bolts to 12 N·m (106 lb in).

6. Install the oil pan baffle (2).
7. Install the oil pan baffle to oil pan retaining bolts (1).

Tighten
Tighten the bolts to 12 N·m (106 lb in).