For 1990-2009 cars

1. Remove all electrical connectors (1-6) from the electrical components.

For Transmission with input speed sensor, disconnect electrical connector (7).

2. Remove the torque converter clutch (TCC/PWM) pulse width modulation retainer clip (395).
3. Remove the TCC/PWM solenoid (396).
4. Remove the TCC solenoid retaining bolts (68).
5. Remove the TCC solenoid and wiring harness (66). Turn the wiring harness over so that it hangs over the side of the transmission.
6. Remove the transmission fluid pressure (TFP) manual valve position switch assembly retaining bolts (62, 70).
7. Remove the TFP manual valve position switch (69).
8. Remove the manual detent spring retaining bolt (64).
9. Remove the manual detent spring assembly (63).
10. Remove all valve body retaining bolts (62).
11. Lift the valve body carefully so that the checkballs remain on the spacer plate in the correct location. While lifting the valve body, disconnect the manual valve link (89) from the manual valve (340).

Notice: Refer to General Repair Instructions in the Preface section.

Important: Some models do not use a #5 ball check valve.

12. Remove the 7 valve body ball check valves (2-6, 8, and 12).
13. Remove the accumulator cover retaining bolts (58, 59 or 117, 118).
14. Remove the 1-2 accumulator cover and pin assembly (57) or 1-2 accumulator cover assembly (116), and gasket (114).

Important: Some models may not use a 1-2 accumulator spring - inner (104) or outer (54).

15. Disassemble the 1-2 accumulator assembly (54, 56, 57, 104).
16. Remove the spacer plate support retaining bolts (77).
17. Remove the spacer plate support (53 or 113).

Important: Some models use a spacer plate (48) with bonded gasket material.

18. Remove the valve body gasket (52), the valve body spacer plate (48) and the case gasket (47).

Discard gaskets. Do not reuse.

Important: Some models do not use a 3-4 accumulator spring (46).

19. Remove the 3-4 accumulator spring (46) and the 3-4 accumulator piston (44).

Notice: Refer to General Repair Instructions in the Preface section.

20. Remove the #1 case ball check valve.