For 1990-2009 cars

The following approximate capacities are given in English and metric conversions. See Fluid and Lubricant Recommendations, for more information. All capacities are approximate. When adding, be sure to fill to the approximate level, as recommended in this manual. Re check fluid level after filling.

Application | Specification
--- | ---
Metric | English
Cooling System

- 3.6L Engine

10 Litres

8.8 Quarts

- 6.0L Engine

11 Litres

9.7 Quarts

Engine Oil with Filter

- 3.6L Engine

6.5 Litres

5.7 Quarts

- 6.L0 Engine

8.3 Litres

7.3 Quarts

Fuel Tank | 73 Litres | 16 Gallons
Automatic Transmission

- 5L40E 5-Speed - Drain and Refill

6 liters

5.3 quarts

- 4L60E 4-Speed - Drain and Refill

4.8 Litres

4.22 Quarts

- 6L80E 6-Speed - Drain and Refill

5.7 Litres

6.0 Quarts

- 5L40E 5-Speed - Complete Overhaul

8.5 Liters

7.4 Quarts

- 4L60E 4-Speed - Complete Overhaul

7.9 Litres

7 Quarts

- 6L80E 6-Speed - Complete Overhaul

9.9 Litres

8.7 Quarts

- 5L40E 5-Speed - Dry

8.5 Liters

7.4 Quarts

- 4L60E 4-Speed - Dry

7.9 Litres

7 Quarts

- 6L80E 6-Speed - Dry

9.9 Litres

8.7 Quarts

Manual Transmission |  |

- D173 6-Speed

1.8 liters

1.6 quarts

- Tremec T56 6-Speed

3.9 liters

3.4 quarts

Differential

- Drain and Fill With Cover Removed

1.2 liters

1 quart

- Drain and Fill With Use of Drain Plug

1.0 liters

0.88 quarts