For 1990-2009 cars

## Windshield Wiper Arm Replacement RHD

### Removal Procedure

Important: Make sure that the wiper arms do not interfere with the bonnet while being moved away from the windshield otherwise damage to the bonnet may occur.

1. Open the Bonnet
2. Remove the wiper arm to pivot stud retaining nut covers (2).
3. Remove the wiper arm to air inlet grille washer hose connectors (3).
4. Remove the wiper arm to pivot stud retaining nuts (1).

Important: Make sure that the wiper arms do not interfere with the bonnet while being moved away from the windshield otherwise damage to the bonnet may occur.

5. Close the Bonnet
6. Lift the wiper arms (1) away from the windshield to the upright position.
7. Remove the LHS wiper arm (4) from the wiper pivot stud.

Important: Make sure that the RHS wiper arm does not interfere with the bonnet otherwise damage to the bonnet may occur.

Important: The RHS wiper should be in the vertical position and away from the windshield as shown.

8. Pull the right hand side wiper arm (1) away from the spline
9. Rotate the RHS wiper arm (1) so the bonnet can be opened without hitting the wiper.
10. Open the bonnet.
11. Manoeuvre the RHS wiper arm (1) off the wiper pivot stud and off the vehicle.

### Installation Procedure

Important: Make sure that the RHS wiper arm does not interfere with the bonnet otherwise damage to the bonnet may occur.

Important: The RHS wiper should be in the vertical position and away from the windshield as shown.

1. Install the RHS wiper arm (1) onto the wiper pivot stud.
2. Install the wiper arm to pivot stud retaining nut (2).

Do not fully tighten at this stage.

3. Close the bonnet

Important: Make sure that the wiper arms do not interfere with the bonnet while being moved away from the windshield otherwise damage to the bonnet may occur.

4. Install the LHS wiper arm (1) to the wiper pivot stud.
5. Install the LHS wiper arm to pivot stud retaining nut (2).

Do not fully tighten at this stage.

6. Lower the wiper arms (1) toward the windshield to the lowered position.

Important: When installing the wiper arm, ensure the installation measurements are adhered to otherwise fouling of the inlet panel may occur.

7. Align the wiper arm blades to the inlet panel using the following measurements :

• | Point ' A' 59 mm

• | Point ' B' 29 mm

Notice: Refer to Fastener Notice in the Preface section.

8. Tighten the LHS wiper arm to pivot stud retaining nut (1).

Tighten
Tighten the nut to 35 N·m (26 lb ft).

9. Open the bonnet.

Notice: Refer to Fastener Notice in the Preface section.

10. Tighten the RHS wiper arm to pivot stud retaining nut (1).

Tighten
Tighten the nut to 35 N·m (26 lb ft).

11. Install the wiper arm to pivot stud retaining nut covers.
12. Connect the wiper arm (3) to the air inlet grille washer hose connectors (4).
13. Close the bonnet.
14. Check the windshield wipers for correct operation.