For 1990-2009 cars

### Remove Procedure

1. Remove the I/P lower trim plate assembly. Refer to Instrument Panel Insulator Panel Replacement - Left Side .
2. Remove the instrument panel outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement in Instrument Panel, Gages, and Console.
3. Remove the I/P compartment assembly. Refer to Instrument Panel Compartment Replacement .
4. Remove the left side floor duct. Refer to Floor Air Outlet Duct Replacement - Left Side .
5. Disconnect the air mix actuator electrical connector (1).
6. Remove the air mix actuator to HVAC module assembly retaining screws (2).
7. Remove the air mix actuator (3) from the HVAC module assembly (4).

### Installation Procedure

1. Install the air mix actuator (3) to the HVAC module assembly (4).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the air mix actuator to HVAC module assembly screws (2).

Tighten
Tighten the screws to 1.5 N·m (13 lb ft).

3. Connect the air mix actuator electrical connector (1).
4. Install left side floor duct. Refer to Floor Air Outlet Duct Replacement - Left Side .
5. Install the I/P compartment assembly. Refer to Instrument Panel Compartment Replacement .
6. Install instrument panel outer trim cover. Refer to Instrument Panel Outer Trim Cover Replacement in Instrument Panel, Gages, and Console.
7. Install the I/P lower trim plate assembly. Refer to Instrument Panel Insulator Panel Replacement - Left Side .
8. Perform HVAC system relearn. Refer to HVAC Control Module Programming and Setup .