For 1990-2009 cars

• | Dirt or debris will cause premature wear of the rebuilt engine. Clean all components. Refer to Cleanliness and Care.

• | Use the correct tools to measure components when inspecting for above acceptable wear. Components that are not within the manufacturers specifications must be repaired or replaced.

• | When the components are installed into an engine, return the components to their original location, position and direction. Refer to Separating Parts.

• | During assembly, lubricate all moving parts with clean engine oil. This provides initial lubrication when the engine is first started.