For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement.
2. Remove the upper auxiliary weatherstrip. Refer to Front Side Door Upper Auxiliary Weatherstrip Replacement.

Important: Use a suitable tool to pry open inner panel (1).

3. Remove the inner panel (1) from the door (2).
4. Disconnect the mirror to door harness electrical connector (1).

Important: Position aside upper auxiliary weatherstrip to locate the front mirror to door retaining screw.

Important: Support the mirror when removing retaining screws (1).

5. Remove the mirror to door retaining screws (1).
6. Remove the mirror from the door.

### Installation Procedure

1. Position the mirror to the door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the mirror to door retaining screws (1).

Tighten
Tighten the screws to 3 N-m (27 lb in).

3. Connect the mirror to door harness electrical connector (1).

Important: Push the inner panel (1) to attach the retainers.

4. Install the inner panel (1) to the door (2).
5. Install the upper auxiliary weatherstrip. Refer to Front Side Door Upper Auxiliary Weatherstrip Replacement.
6. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement.