For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the transmission support. Refer to Transmission Support Replacement.
3. Remove the transmission mount to transmission upper retaining bolts (2).
4. Remove the transmission mount (1).

### Installation Procedure

1. Install the transmission mount (1) to the transmission.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the transmission mount to transmission upper retaining bolts (2).

Tighten
Tighten the bolts to 60 N·m (44 lb ft).

3. Install the transmission support. Refer to Transmission Support Replacement.
4. Lower the vehicle.