For 1990-2009 cars

## Fastener Tightening Specifications RHD

Application | Specification
--- | ---
Metric | English
Amplifier Mounting Bracket to Vehicle Retaining Bolts | 22 N·m | 16 lb ft
Amplifier to Mounting Bracket Retaining Screws | 2.5 N·m | 22 lb in
Antenna Module Ground Point to Roof Panel Retaining Bolt | 2 N·m | 18 lb in
Antenna Module to Roof Panel Retaining Bolt | 4 N·m | 35 lb in
Backup Battery Cover to Telematics Module Retaining Screws | 2 N·m | 18 lb in
Centre Speaker to Insulation Panel (I/P) Attaching Screws | 2 N·m | 18 lb in
Diversity Antenna Module to Rear Upper Quarter Panel Retaining Bolt | 10 N·m | 89 lb in
DVD Player Surround to Roof Panel Retaining Screw | 1 N·m | 9 lb in
DVD Screen Assembly to Head Restraint Assembly Retaining Screws | 2 N·m | 18 lb in
DVD Screen Surround to Roof Panel Retaining Screw | 1 N·m | 9 lb in
DVD Screen to Mounting Plate Retaining Screws | 2 N·m | 18 lb in
DVD Screen to RSE Assembly Bracket Retaining Screws | 1.5 N·m | 13 lb in
Front Speaker Assembly to Door Frame Attaching Screws | 2 N·m | 18 lb in
Infotainment Unit to Instrument Panel Retaining Screws | 2 N·m | 18 lb in
I/P Compartment Lower Retaining Screws | 2 N·m | 18 lb in
I/P Compartment Upper Retaining Screws | 2 N·m | 18 lb in
Navigation Interface Module (NIM) to I/P Assembly Retaining Screws | 2 N·m | 18 lb in
Pivot Hinge to Mounting Plate Retaining Screws | 2 N·m | 18 lb in
Rear Speaker Assembly to Door Frame Attaching Screws | 2 N·m | 18 lb in
RSE Circuit Board to Head Restraint Assembly Retaining Screws | 2 N·m | 18 lb in
RSE Head Restraint Escutcheon to Head Restraint Assembly Retaining Screws | 2 N·m | 18 lb in
Subwoofer Assembly to Rear Shelf Attaching Screws | 2 N·m | 18 lb in
Telematics Module to Retaining Bracket Retaining Screw | 2 N·m | 18 lb in
Tweeter Speaker to I/P Attaching Screw | 2 N·m | 18 lb in