For 1990-2009 cars

Checks | Causes
--- | ---
4-5-6 (with Turbine Shaft) Clutch Assembly (56) |

• | Inspect for damaged 4-5-6 clutch (with turbine shaft) housing assembly (441).

• | Inspect for damaged or distorted turbine shaft.

1-2-3-4 Clutch (with Output Carrier Inner Sun Gear Shaft) Hub Assembly (61) | Inspect for damaged or distorted shaft on hub assembly.
2-6 and 3-5-R Clutch (with Output Carrier Outer Sun Gear Shaft) Hub Assembly (64) |

• | Inspect for damaged or distorted shaft on hub assembly.

• | Inspect the output carrier inner sun gear shaft bushings (60 and 62) for damage or wear.