For 1990-2009 cars

1. Install the wiring harness connector (55) through the case. Hold the connector and install the wiring harness connector retainer (54).
2. Install the wiring harness to the valve body and connect the following components:

• | Pressure Control Solenoid (357)

• | TCC PWM Solenoid (352)

• | 1-2 Shift Solenoid (368)

• | 2-3 Shift Solenoid (369)

• | 4-5 Shift Solenoid (376)

• | Internal Mode Switch - IMS (602)

• | Input Speed Sensor (44)

• | Output Speed Sensor (42)