For 1990-2009 cars

#### Tools Required

• | J-22912-01 Split Plate

• | J 39473 Mainshaft Bearing Installer

• | J 39511 Split Plate

• | J 39547 Press Adapter

Important: Do not replace tapered bearings unless inspection shows bearing damage.

1. Remove the small tapered bearing (3), using the J-22912-01 (1) with the J 39473 (2) and a hydraulic press.
2. Discard the small tapered bearing (3).
3. Remove the large tapered bearing (2), using the J 39511 (3), the J 39547 (1), and a hydraulic press.
4. Discard the large tapered bearing (2).