For 1990-2009 cars

### Removal Procedure

Important: Pull the rear compartment weatherstrip (2) from the rear compartment pinch-weld flange (1).

1. Remove the rear compartment weatherstrip (2) from the pinch-weld flange (1).
2. Remove the rear compartment weatherstrip (2) from the vehicle.

### Installation Procedure

1. Position the rear compartment weatherstrip (2) over the top of the rear compartment pinch-weld flange (1).

Important: Press the rear compartment weatherstrip (2) onto the rear compartment pinch-weld flange (1) and make sure that the rear compartment weatherstrip (2) is secured correctly to the entire pinch-weld flange (1).

2. Install the rear compartment weatherstrip (2) to the pinch weld flange (2).