For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
2 Bearing Retaining Bolts M14x135 (2x) | 153 N-m | 112 lb ft
2 Bearing Retaining Bolts M14x100 (2x) | 153 N-m | 112 lb ft
6 Differential Housing Retaining Bolts M10x1.5x75 (6x) | 53 N-m | 39 lb ft
10 Ring Gear Retaining Bolts M12 (10x) | 125 N-m | 92 lb ft
Pinion Flange Nut (In Vehicle) | Record pinion drag torque before removal and torque to the same value on installation. | Record pinion drag torque before removal and torque to the same value on installation.
Pinion Flange Nut (Out of Vehicle) | 2.5 N-m | 23 Ib in
Differential Fill Plug | 35 N-m | 26 lb ft
Differential Drain Plug | 35 N-m | 26 lb ft
Breather Fitting | 15 N-m | 11 lb ft
Differential to Subframe Retaining Nuts | 80 N-m | 59 lb ft