For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the exhaust system. Refer to Exhaust System Replacement.
3. Remove the right catalytic converter. Refer to Catalytic Converter Replacement - Right Side.
4. Remove the transmission vent tube to transmission case retaining bolt (1).
5. Remove the transmission vent tube from the vent pipe.

### Installation Procedure

1. Install the transmission vent tube to the vent pipe.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the transmission vent tube to transmission case retaining bolt (1).

Tighten
Tighten the transmission vent tube retaining bolt to 48 N·m (35 lb ft).

3. Install the right catalytic converter. Refer to Catalytic Converter Replacement - Right Side.
4. Install the exhaust system. Refer to Exhaust System Replacement.
5. Lower the vehicle.