For 1990-2009 cars

#### Tools Required

• | J 41510 T-50 Plus Bit.

• | DT-49362 Mortorq Bit.

Important: Ensure converter housing and case face are clean before installing new pump seal.

Important: When installing a new oil pump seal (5), the seal will protrude slightly above the case surface. The oil pump seal is a wedge design that will conform to the surfaces between the oil pump body and the transmission case as the converter housing (105) is installed.

1. Install the oil pump seal (5). Seat oil pump seal (5) by hand, between pump body and case. Ensure the seal is evenly seated.
2. Install the converter housing (102).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the converter housing retaining bolts (94) to the transmission case. Use the J 41510 or DT-49362 .

Tighten
Tighten the converter housing retaining bolts (94) to 65-75 N·m (48-55 lb ft).

Tighten converter housing retaining bolts evenly in a star pattern sequence.