For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Remove the cargo liner. Refer to Cargo Box Liner Replacement .

Important: The soft tonneau cover support bow bracket retaining rivets and washers are single use parts. They must be discarded after removal.

2. Drill out the soft tonneau cover support bow bracket to cargo liner retaining rivets (2).

Discard the rivets.

3. Remove the soft tonneau cover support bow bracket (3) from the cargo liner (1).

### Installation Procedure

1. Position the soft tonneau cover support bow bracket (3) to the cargo liner (1).

Important: The soft tonneau cover support bow bracket retaining NEW rivets and washers must be installed to make sure of correct bedliner retention.

2. Install NEW soft tonneau cover support bow bracket retaining rivets and washers (2) to the soft tonneau cover support bow bracket (1) using a suitable tool.
3. Install the cargo liner. Refer to Cargo Box Liner Replacement .