For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Open and suitably support the liftgate.
3. Disconnect liftgate door grommet.
4. Disconnect the electrical connector.
5. Disconnect the liftgate washer hose.
6. Remove the liftgate struts. Refer to Liftgate Strut Replacement .
7. With the aid of an assistant, remove the bolts and the liftgate from the hinges.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. With the aid of an assistant, install the liftgate to the hinges with the bolts.

Tighten
Tighten the liftgate bolts to 20 N·m (15 lb ft).

2. Install the liftgate struts. Refer to Liftgate Strut Replacement .
3. Connect the liftgate washer hose.
4. Connect the electrical connector.
5. Connect the liftgate door grommet.
6. Connect the negative battery cable.