For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Remove the valve body assembly. Refer to Control Valve Body Replacement .
2. Pull out the sealing sleeve (Brake C) using a nail.
3. Turn the transaxle by 90 degrees.
4. Remove the rear cover bolts.
5. Loosen the cover by tapping firmly on the side of the cover.
6. Remove the cover.

### Installation Procedure

1. Install the rear cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear cover bolts.

Tighten
Tighten the bolts to 23 N·m (17 lb ft).

3. Turn the transaxle by 90 degrees.
4. Install the sealing sleeve (Brake C).
5. Install the valve body assembly. Refer to Control Valve Body Replacement .