For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Crossmember-to-Body Bolts | 112 N·m | 83 lb ft
Front Parallel Link-to-Knuckle Bolt | 120 N·m | 89 lb ft
Fuel Filler Hose Shield Bolt | 20 N·m | 15 lb ft
Knuckle-to-Strut Assembly Nuts | 100 N·m | 74 lb ft
Rear Hub Assembly Bolts | 65 N·m | 48 lb ft
Rear Parallel Link-to-Crossmember Bolt | 90 N·m | 66 lb ft
Rear Parallel Link-to-Knuckle Bolt | 90 N·m | 66 lb ft
Rear Trailing Link-to-Knuckle Nut | 150 N·m | 111 lb ft
Rear Trailing Link-to-Trailing Link Bracket Nut | 100 N·m | 74 lb ft
Stabilizer Link-to-Strut Assembly Nut | 47 N·m | 35 lb ft
Stabilizer Shaft Clamp Bolts | 40 N·m | 30 lb ft
Stabilizer Shaft-to-Stabilizer Link Nut | 47 N·m | 35 lb ft
Strut Dampener-to-Strut Mount Nut | 75 N·m | 55 lb ft
Strut Mount-to-Body Nuts | 30 N·m | 22 lb ft
Trailing Link Bracket-to-Body Bolts | 70 N·m | 52 lb ft
Trailing Link-to-Trailing Link Bracket Nut | 100 N·m | 74 lb ft