For 1990-2009 cars

### Removal Procedure

1. Remove the nuts securing the lock cylinder.
2. Disconnect the lock rod.
3. Disconnect the electrical connector.
4. Remove the rear compartment lock cylinder.

### Installation Procedure

1. Install the rear compartment lock cylinder.
2. Connect the electrical connector.
3. Connect the lock rod.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the rear compartment lock cylinder with the nuts.

Tighten
Tighten the rear compartment lock cylinder nut to 8 N·m (71 lb in).