For 1990-2009 cars

### Removal Procedure

Important: Install protective coverings over the fenders and the windshield in order to prevent damage to the paint, the glass, and the moldings when you are removing and installing the hood.

1. Raise and support the hood.
2. Mark the position of the hinge to the hood to facilitate alignment during installation.
3. Remove the bolts that retain the hood to both hinges.
4. With the aid of another technician, remove the hood from the hinges.

### Installation Procedure

1. With the aid of another technician, position the hood in the location marked during removal.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the 2 bolts securing the hood to each hinge.

Tighten
Tighten the hood-to-hinge bolts to 27 N·m (20 lb ft).

3. Inspect the hood for proper alignment.