For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the wheel. Refer to Tire and Wheel Removal and Installation.
3. On vehicles equipped with rear drum brakes, remove the rear brake drum detent screw and brake drum. Refer to Drum Brake Adjustment.
4. On vehicles equipped with rear disc brakes, remove the rear brake caliper and rear brake disc. Refer to Rear Brake Caliper Replacement.
5. Remove the hub bolts and hub assembly.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the hub assembly bolts and tighten to 65 N·m (48 lb ft).
2. Install the hub nut.
3. On vehicles equipped with rear disc brakes, install the rear brake disc and rear brake caliper. Refer to Rear Brake Caliper Replacement.
4. On vehicles equipped with rear drum brakes, install the rear brake drum and the brake drum detent screw. Refer to Drum Brake Adjustment.
5. Install the wheel. Refer to Tire and Wheel Removal and Installation.
6. Lower the vehicle.