For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Mark the position of the hood latch on the radiator support to facilitate alignment during installation.
3. Remove the bolts and the hood latch.

### Installation Procedure

1. Position the hood latch in the location marked during removal.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the hood latch with the bolts.

Tighten
Tighten the hood latch bolts to 8 N·m (71 lb in).