For 1990-2009 cars

1. Perform a preliminary inspection before any attempt is made to change or correct the wheel alignment factors. Refer to Preliminary Alignment Inspection .
2. Loosen the front parallel link cam bolt to crossmember.

Notice: Refer to Fastener Notice in the Preface section.

3. Rotate the parallel link adjustment bolts until the preferred rear toe specification is obtained. Refer to Wheel Alignment Specifications .

Tighten
Tighten the bolt to 40 N·m (30 lb ft).

4. Hold the parallel link adjustment bolts and tighten the parallel link-to-crossmember nuts.

Tighten
Tighten the parallel link-to-crossmember nuts to 90 N·m (66 lb ft).