For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Blower Motor Resistor Screws | 1.2 N·m | 11 lb in
Blower Motor Retaining Screws | 1.2 N·m | 11 lb in
Blower Motor-to-A/C Assembly Screws | 1.2 N·m | 11 lb in
Compressor-Clutch Plate and Hub Assembly Retaining Nut | 17 N·m | 13 lb ft
Compressor-Through Bolts | 10 N·m | 89 lb in
Compressor-to-Bracket Mounting Bolts - 1.4L, 1.6L and 2.0L Diesel only | 27 N·m | 20 lb ft
Condenser Mount Bolts | 4 N·m | 35 lb in
Controller Retaining Screws | 2 N·m | 18 lb in
Evaporator Core Cover Screws | 1.2 N·m | 11 lb in
Expansion Valve Stud Bolts | 8 N·m | 71 lb in
Front Compressor-to-Bracket Mounting Bolts - 1.8L, 2.0L only | 35 N·m | 26 lb ft
Heater Core Cover Screws | 1.2 N·m | 11 lb in
Heater Core Housing-to-Evaporator Housing Screws | 1.2 N·m | 11 lb in
Heater/Air Distributor Case Assembly Screw | 4 N·m | 35 lb in
Liquid Pipe Block-to-Expansion Valve Retaining Nut | 14 N·m | 10 lb ft
Liquid Pipe Block-to-Receiver Dryer Retaining Nut | 14 N·m | 10 lb ft
Liquid Pipe Support Clamp Bolts | 8 N·m | 71 lb in
Pressure Transducer | 7 N·m | 62 lb in
Rear Compressor-to-Bracket Mounting Bolts - 1.8L, 2.0L only | 20 N·m | 15 lb ft
Receiver Dryer - Band Clamp Bolt | 5 N·m | 44 lb in
Receiver Dryer-to-Condenser Pipe Block Bolt | 5 N·m | 44 lb in
Refrigerant Discharge Hose Block-to-Compressor Retaining Nut | 33 N·m | 24 lb ft
Refrigerant Discharge Hose Block-to-Condenser Retaining Nut | 16 N·m | 12 lb ft
Suction Hose Block-to-Compressor Retaining Nut | 33 N·m | 24 lb ft
Suction Hose Block-to-Expansion Valve Retaining Nut | 14 N·m | 10 lb ft
Suction Hose Support Clamp-to-Engine Bracket Bolt - 1.4L, 1.6L and 2.0L Diesel | 8 N·m | 71 lb in
Suction Hose Support Clamp-to-Engine Bracket Bolt - 1.8L, 2.0L only | 14 N·m | 10 lb ft
Suction Hose Support Clamp-to-Longitudinal Member Bolt | 8 N·m | 71 lb in