For 1990-2009 cars

1. Perform a preliminary inspection before any attempt is made to change or correct the wheel alignment factors. Refer to Preliminary Alignment Inspection.
2. Loosen the front parallel link cam bolt to crossmember.

Caution: Refer to Fastener Caution in the Preface section.

3. Rotate the parallel link adjustment bolts until the preferred rear toe specification is obtained, then tighten to 40 N·m (30 lb ft). Refer to Wheel Alignment Specifications.
4. Hold the parallel link adjustment bolts, install the parallel link-to-crossmember nuts and tighten to 90 N·m (66 lb ft).