For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the headlamp. Refer to Headlamp Replacement .
3. Disconnect the electrical connector.
4. Remove the side marker lamp.

### Installation Procedure

1. Connect the electrical connector.
2. Install the side marker lamp.
3. Install the headlamp. Refer to Headlamp Replacement .
4. Connect the negative battery cable.