For 1990-2009 cars

### Removal Procedure

With the aid of an assistant, remove the bolts and the hinge from the door and the body.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

With the aid of an assistant, install the hinge to the door and the body with the bolts.

Tighten

• | Tighten the door hinge-to-body bolts to 20 N·m (15 lb ft).

• | Tighten the door hinge-to-door bolts to 20 N·m (15 lb ft).