For 1990-2009 cars

Checks | Actions
--- | ---
Inspect the intermediate shaft shield for interference with the steering gear dust cover. | Replace the intermediate shaft.
Inspect the steering gear for a squeak or growl noise while turning the steering wheel to the left or to the right. | Replace the steering gear.
Inspect the steering gear-to-column joints for improper installation. | Tighten the steering shaft universal joint pinch bolts. Replace as needed.
Inspect the steering shaft bearing for wear or damage. | Replace the steering shaft bearing.
Inspect the spherical joint for lack of lubrication. | Lubricate the spherical joint.
Inspect the steering shaft for lack of lubrication. | Lubricate the steering shaft.
Inspect the shaft lock snap ring for improper seating. | Adjust the shaft lock snap ring. Replace the shaft lock snap ring as needed.