For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the electrical connector.
3. Remove the bolt and the horn.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the horn with the bolt.

Tighten
Tighten the horn bolt to 20 N·m (15 lb ft).

2. Connect the electrical connector.
3. Connector the negative battery cable.