For 1990-2009 cars

DTC | Description | Type* Non European Emissions | Type* European Emissions
--- | --- | --- | ---
P0562 | DTC P0562 | C2 | B
P0563 | DTC P0563 | C2 | B
P0601 | DTC P0601 | C1 | A
P0604 | DTC P0604 | C2 | B
P0705 | DTC P0705 | C2 | B
P0712 | DTC P0712 | C1 | A
P0713 | DTC P0713 | C1 | A
P0717 | DTC P0717 | C1 | A
P0722 | DTC P0722 | C1 | A
P0727 | DTC P0727 | C1 | A
P0741 | DTC P0741 | C2 | B
P0742 | DTC P0742 | C2 | B
P0743 | DTC P0743 | C2 | B
P0748 | DTC P0748 | C1 | A
P0751 | DTC P0751 | C2 | B
P0753 | DTC P0753 | C1 | A
P0756 | DTC P0756 | C2 | B
P0758 | DTC P0758 | C1 | A
P0785 | DTC P0785 | C1 | A
P1781 | DTC P1781 | C1 | A
P1791 | DTC P1791 | C1 | A
P1792 | DTC P1792 | D | D
U2105 | DTC U2105 | C1 | A
*Description of Type

• | Type A: The transmission control module (TCM) will request the illumination of the malfunction indicator lamp (MIL) lamp and store a DTC when the TCM detects a failure on the first ignition cycle.

• | Type C1: The TCM will request the illumination of the hold lamp and store a DTC when the TCM detects a failure on the first ignition cycle.

• | Type B: The TCM will request the illumination of the MIL and store a DTC when the TCM detects failures on 2 consecutive ignition cycles.

• | Type C2: The TCM will request the illumination of the hold lamp and store a DTC when the TCM detects failures on 2 consecutive ignition cycles.

• | Type D: The TCM will not request the illumination of the MIL or hold lamp, but will store a DTC when the TCM detects a failure on the first ignition cycle.