For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the return spring from the clutch pedal.
3. Remove the clip and the pedal mounting shaft.
4. Remove the locking clip and push rod fixing pin.
5. Remove the push rod from the clutch pedal.
6. Remove the clutch pedal.

### Installation Procedure

1. Install the clutch pedal.
2. Coat the push rod with multi-purpose grease.
3. Install the push rod to the clutch pedal.
4. Install the locking clip and push rod fixing pin.
5. Coat the pedal mounting shaft with multi-purpose grease.
6. Install the clip and the pedal mounting shaft.
7. Connect the return spring to the clutch pedal.
8. Adjust the clutch pedal play. Refer to Clutch Pedal Free Travel Adjustment.
9. Connect the negative battery cable.