For 1990-2009 cars

#### Tools Required

J 28467-B (DW117) Universal Engine Support Fixture

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Remove the battery.
2. Install J 28467-B (1).
3. Remove the left transaxle mounting bolts.
4. Remove the cage bolts (1, 3) and nut (2) from the left transaxle mounting bracket.
5. Remove the mounting bracket.

### Installation Procedure

1. Install the left transaxle mounting bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the cage bolts (1, 3) and nut (2) to the mounting bracket.

Tighten

• | Tighten the bolt (3) to 110 N·m (81 lb ft).

• | Tighten the bolt (1) to 65 N·m (48 lb ft).

• | Tighten the nut (2) to 65 N·m (48 lb ft).

3. Install the left transaxle mounting bolts.

Tighten
Tighten the bolts to 48 N·m (35 lb ft).

4. Remove J 28467-B (1).
5. Install the battery.