For 1990-2009 cars

### Removal Procedure

1. Remove the power steering pump from the engine. To remove the actuator, it is necessary that the power steering pump be removed from the engine. Refer to Power Steering Pump Replacement for removal of the power steering pump from the engine.

Important: Note the positioning of the electrical connector and discharge fitting before removal. Noted positions will be used during installation.

2. Remove the position-retaining clip from the power steering pump actuator.
3. Remove the actuator and discharge fitting from the power steering pump.
4. Remove and discard the actuator O-rings.

### Installation Procedure

1. Install the discharge fitting and power steering pump actuator with new O-rings to the power steering pump.

Notice: Refer to Fastener Notice in the Preface section.

2. Position the discharge fitting to noted location during disassembly.

Tighten
Tighten the actuator to 62 N·m (46 lb ft).

3. Install the position-retaining clip to the actuator using noted connector positioning during disassembly.
4. Install the power steering pump to the engine. Refer to Power Steering Pump Replacement .
5. Connect the actuator electrical connector.
6. Perform the Diagnostic System Check.